December 24, 2020

Minority Business Development Center

47 Market Street, Room 808

Tacoma, WA 98402

**DBE Subcontractor Solicitation for Bids or Proposals for Public Utility District No. 1 of Skagit County, Judy Reservoir to Mount Vernon Transmission Pipeline – Phase 2**

**Business Name (Prime Contractor):** Michels Corporation

**Type of Businesses Being Solicited:** Women-Owned Small Business,Disadvantaged Business Enterprise (DBE), Small Business with Top Secret Security Clearance/Sensitive Compartmented Information (TS/SCI), Small Business with Top Secret Security Clearance (TS), Small Business with Secret Security Clearance (SC), Small Business (SB), SBA Certified HUBZone Small Business (HUBZone SB), SBA Certified 8a Program Participant, Small Disadvantaged Business (SDB), Women-Owned Small Business under the SBA Women-Owned Small Business Program, Economically Disadvantaged Women-Owned Small Business, Veteran-Owned Small Business (VOSB), Service-Disabled Veteran-Owned Small Business (SDVOSB), Alaskan Native Corporations (ANC) and Indian Tribe, Tribally Owned, Native Hawaiian Org (NHO) Owned, Economically Disadvantaged Women-Owned Small Business under the Women-Owned Small Business Program, Women-Owned Small Business Joint Venture, Economically Disadvantaged Women-Owned Small Business Joint Venture

**NAICS Code:** 237110 Water and Sewer Line and Related Structures Construction

**Additional NAICS Codes:** 524126; 238910; 541820; 238110; 541330; 541690; 237990; 236220; 238210; 561730; 238990; 237310; 237110

**Solicitation Description:** Construction of 5.3 miles of 36-in diameter welded steel water transmission pipeline, 75 LF of 8-in diameter ductile iron pipe installed within an 18-in diameter steel casing installed by bored and jacked casing methods, dewatering to allow open trenching and pipe installation, new fish-passable precast concrete box culvert, new 220 LF single span steel truss bridge, installation of two 36-in diameter flow meters in vaults, electrical and SCADA at the Judy Reservoir Water Treatment Plant, installation of a 4-in diameter fiber optic conduit for the entire alignment of the 36-in diameter water transmission pipeline, 2.3 miles of Service Road along transmission pipeline including grading and installation of storm culverts and drain piping.

**Solicitation Point of Contact:** Dawson Dionne, 920-573-0189, [ddionne@michels.us](mailto:ddionne@michels.us)

**Place of Performance:** Mount Vernon, WA, Clear Lake, WA, Skagit County, WA

**Performance Start Date:** March 31, 2021

**Solicitation Closing Date:** January 26, 2021

**Solicitation Number:** P.N. 3549; C.O. 4385